e-radionica Maker LED Display Library



Initializing Library

Must call this function before calling any other function from class.

It initializes IS31FL3731 Led Driver and sets up IS31FL3731 library to work with this board. First you have to download and install IS31FL3731 libarary!

int Maker\_LED\_Matrix\_32::begin(void);

Parameters: None

Returns:

1 For successful initialization

0 For unsuccessful initialization

NOTE: If is initialization unsuccessful, user defined program should not continue!

Setting up font and background brightness

This function enables user to set desired brightness level for fonts and for background.

void Maker\_LED\_Matrix\_32::brightness(uint8\_t \_fontLight, uint8\_t \_backingLight);

Parameters:

uint8\_t \_backingLight - Sets up a brightness of background. It goes from 0 (dark) to 255 (bright). If user don't want background to light up, set this to zero.

Returns: None

Displaying a message on display

With this function, user can send a message to display. It can also set does want to scroll that message, or not and also how fast to do scrolling.

void Maker\_LED\_Matrix\_32::message(char\* msg, int \_ms, int \_stp, int \_rep);

Parameters:

char\* msg - String (message) that will be displayed on display.

int \_ms - Integer that set how long is delay in milliseconds between two scroll steps (shifts). It must be larger than 10 ms.

int \_stp - Integer that set how many pixels will be skipped in just one step in scrolling. Must not be negative or zero.

int \_rep - Integer that determine how many times message have repeated on display. -1 means that message will scroll all the time, 0 means that message will be stationary (no scrolling).

Returns: None.

Stopping scrolling message on display

Calling this function, message that is displayed on panel, will be stopped from scrolling. You can continue scrolling by calling Maker\_LED\_Matrix\_32::resumeScroll(void) function.

void Maker\_LED\_Matrix\_32::stopScroll(void);

Parameters: None.

Returns: None.

Resuming scrolling

Calling this function, message that is previously stopped from scrolling by calling Maker\_LED\_Matrix\_32::stopScroll(void) function, will continue to scroll.

void Maker\_LED\_Matrix\_32::resumeScroll(void);

Parameters: None.

Returns: None.

Deleting message or picture form screen

Calling this function, everything on display will be deleted. Also, it will delete everything from buffers inside the library.

void Maker\_LED\_Matrix\_32::deleteScroll(void);

Parameters: None.

Returns: None.

Drawing 8x8 pixels bitmap image on screen

This function enables user to display bitmap picture on specific location on screen. This picture is not scrolling.

void Maker\_LED\_Matrix\_32::picture(uint8\_t\* p, int posX, int posY);

Parameters:

uint8\_t\* p - Address to bitmap picture.

int posX - Sets x coordinate of picture.

int posY - Sets y coordinate of picture.

Returns: None.

**NOTE:** Bitmap has to be 8x8 pixels!

Scrolling bitmap picture on screen

With this function, user can send a bitmap picture that will scroll on display. It will delete everything that was previously been on display.

void Maker\_LED\_Matrix\_32::scrollPicture(uint8\_t\* p, int \_ms, int \_stp);

Parameters:

uint8\_t\* p - Address to bitmap picture.

int \_ms - Integer that set how long is delay in milliseconds between two scroll steps (shifts). It must be larger than 10 ms.

int \_stp - Integer that set how many pixels will be skipped in just one step in scrolling. Must not be negative or zero.

Returns: None

**NOTE:** Bitmap has to be 8x8 pixels!

Scrolling message along with picture

With this function, user can display text and bitmap pictures at the same time. It will clear all that was previously been on display.

void Maker\_LED\_Matrix\_32::scrollTxtAndPics(char\* txt, uint8\_t\*\* p, uint16\_t\* picsPos\_x, uint16\_t\* picsPos\_y, uint8\_t n, int \_ms, int \_stp, int \_rep);

Parameters:

char\* txt - String that user wants to display on screen.

**NOTE**: There must be two blank spaces on position where picture needs to be!

uint8\_t\*\* p - Address of field of pointers that consists of bitmap picture addresses. It has to be in exact order that will be displayed on display.

uint16\_t\* picsPos\_x - Pointer to field of x coordinates for each picture. In same order as on uint8\_t\*\* p.

uint16\_t\* picsPos\_y - Pointer to field of y coordinates for each picture. In same order as on uint8\_t\*\* p.

uint8\_t n - Number of pictures in message.

int \_ms - Integer that set how long is delay in milliseconds between two scroll steps (shifts). It must be larger than 10 ms.

int \_stp - Integer that set how many pixels will be skipped in just one step in scrolling. Must not be negative or zero.

int \_rep - Integer that determine how many times message have repeated on display.

-1 means that message will scroll all the time, 0 means that message will be stationary (no scrolling).

Returns: None.

**NOTE:** Bitmap has to be 8x8 pixels!

Counting how may times message has been repeated on screen

This function keeps track on how many times has message been repeated on screen. Useful if user wants to wait until the message is whole displayed.

int Maker\_LED\_Matrix\_32::repeatCount(void);

Parameters: None.

Returns: Number of times that message has been repeated on screen.

Displaying a greyscale picture on screen

Using this function, user can display 8-bit greyscale image on screen. Picture should be stored in one dimensional array with element size of 8 bits wide.

void Maker\_LED\_Matrix\_32:: picture8Bit(uint8\_t\* p, int xSize, int ySize, int x0, int y0, uint8\_t bright);

Parameters:

uint8\_t\* p - Pointer to array (picture). Element in this array must me 8 bits.

int xSize - Size of picture (pixels) in x direction.

int ySize - Size of picture (pixels) in y direction.

int x0 - X coordinate of picture (point 0,0 of picture is upper left).

int y0 - Y coordinate of picture (point 0,0 of picture is upper left).

uint8\_t bright - Sets the brightness of picture (it uses Gamma correction for brightness). Gamma factor is 2.2 and can be changed by opening header file of this library.

Returns: None

Connecting to WLAN Network

Use this function to connect to WLAN network for accessing the Internet.

int Maker\_LED\_Matrix\_32::wifiNetwork(const char\* \_ssid, const char\* \_pass);

Parameters:

const char\* \_ssid - String that contains WLAN network name.

const char\* \_pass - String that contains password of WLAN network.

Returns:

1 For successful connection to WLAN network.

0 For unsuccessful connection to WLAN network.

Display web page content on LED Matrix

Use this function for opening specific web page and displaying one line of text on display.

int Maker\_LED\_Matrix\_32::webPage(char\* web, char\* url, int port, int \_ms, int \_stp, int \_rep);

Parameters:

char\* web - String that contains name of web client (example: www.google.com).

char\* url - String that contains URL of the user defined Web page that has text that has to be displayed on screen.

int port - Port of the web client for specific application. (In case of web page usually is 80, 88, 8080).

Returns:

1 For successful connecting to client and opening web page.

0 For unsuccessful connecting to client or opening web page.

Getting web page content

Use this function to catch one line of text from web page. It will not display it on screen.

int Maker\_LED\_Matrix\_32::webPageText(char\* web, char\* url, int port, char\* txt, int \_n);

Parameters:

char\* web - String that contains name of web client (example: www.google.com).

char\* url - String that contains URL of the user defined Web page.

int port - Port of the web client for specific application. (In case of web page usually is 80, 88, 8080).

char\* txt - Pointer to string in which text from web page will be saved.

int \_n - Number of letters (elements of string) that user wants to copy into string.

Returns:

1 For successful connecting to client and opening web page.

0 For unsuccessful connecting to client or opening web page.